{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["RK-02-2003-02, př. 2"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"RK-02-2003-02, př. 2","index":0,"n_rows":55,"n_cols":6,"rows_kept":55,"cut":false,"hidden":false,"merged":[[19,0,19,2],[3,1,4,2],[3,0,4,0],[0,0,0,5]],"flags":["formulas_cached_only"]}
["PŘÍLOHA 11:  INVESTIČNÍ AKCE NA SILNICÍCH II. A III. TŘÍDY"]
[]
[]
["číslo silnice","akce",null,"celkové",2002,2003]
[null,null,null,"náklady"]
["III/3924","Holubí Zhoř","reko mostu",4400]
["III/11226","Blažnov","oprava mostu",6000]
["II/112","Červená Řečice","bodová závada",1200]
["II/360","Radešínská Svratka","bodová závada",6000]
["II/360","Moravec"]
["II/388","Zvole"]
["II/409","Panské Dubenky","přeložka mostu",7500]
["II/352","Polná","přeložka",6000]
["III/4066","Třešť","oprava mostu",8000]
["III/3456","Golčův Jeníkov","rekonstrukce silnice",3557]
["II/408","Jemnice","havárie svahů",4650]
["III/38815","Vír-Hluboké","technický dozor",150]
["II/150","Hněvkovice","rozšíření silnice",213]
[null,"Projektová dokumentace","příprava",2000,null,2000]
["Celkem",{"$nulls":4},33303]
{"$rows_empty":34}
[null,null,"Strana 1"]