{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["RK-31-2001-12, př. 1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"RK-31-2001-12, př. 1","index":0,"n_rows":11,"n_cols":16,"rows_kept":11,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
[{"$nulls":14},"RK-31-2001-12, př. 1"]
[{"$nulls":14},"počet stran: 1"]
["Poř.č.","Sil.","Okres","Akce","Staničení","Šířka m","Délka km","m2 ts.","Kč/m2","Cena silnice tis.Kč","Cena mostů tis.Kč","Dopravní zatížení","Typ poruchy","Typ opravy","Počet mostů","evid.č. mostů"]
[null,"II/405","TR","hr. okresu křiž. III/40512 Petrovice","110,031 - ",7.5,9.429,70717,345,24400,0,"1991 -3769","příčné deformace,výtluky, nerovnosti","frézování, vyrovnání,ABS5",0]
[null,"II/360","TR","hr.okresu, Štěpkov, kř. Vacenovice, Jaroměřice n/R","110,031 - 141,636",7.5,31.605,237037,443,105000,7900,"2693 -13657","příčné deformace,výtluky, nerovnosti","frézování, vyrovnání,ABS5",6,"048, 049, 050, 051 053, 058"]
[null,"II/406, II/112","JI","kř. II/602 -Třešť -Telč","0,000-10,540 11,112-23,484",7.5,22.902,171765,756,130000,null,"1870 -4459","deformace, výtluky, rozšížení na 7,5","frézování, zesílení konstrukce",3,"000a, 002, 005"]
[null,"II/353, II/602","JI","D1 -V.Beranov - Dvorce","63,222 -66,462 75,772 - 88,077",7.5,15.545,116587,450,52200,null,"3195 - 9408","deformace, výtluky, trhliny","frézování, zesílení konstrukce",3,"040, 041, 042"]
[null,"II/345","HB","Chotěboř - Golčův Jeníkov","0,750 -19,764","6,5 - 8",19.014,140163,650,91106,1220,null,"podélné deformace, trhliny, plošný rozpad vozovky","frézování, nový živičný kryt",4,"001,002,003,005"]
[null,"II/150","HB","Havlíčkův Brod - Ledeč n/S.","51,820 -87,175","6,1 - 7,5",35.355,240608,650,156395,3340,null,"podélné deformace, trhliny, plošný rozpad vozovky","frézování, nový živičný kryt 10 cm",6,"015,019,020,021,022,023"]
[null,"II/375","ZR","Jimramov - Ubušínek","0,580 -5,300",6,4.72,28320,320,9060,0,256,"úplný rozpad vozovky","OKS51AB5",0]
[null,"II/388","ZR","Vír - Rovečné","42,664 - 48,075",6,5.411,32466,320,10390,0,648,"úplný rozpad vozovky","OKS51AB5",0]